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SPHERICAL POWDER FOR THE MANUFACTURE OF PARTS USING SELECTIVE LASER MELTING (SLM) TECHNOLOGY IN 3D PRINTERS
NICKEL/STAINLESS/COBALT-CHROME/TITANIUM ALLOYS
	GH4648
	INCONEL 718
	INCONEL 625

	HASTELLOY X
	INCONEL 713
	HAYNES 188

	RENE 95
	WASPALOY
	RENE 125

	MOLYBDENUM  -MO
	TUNGSTEN  W
	TANTALUM TA

	NIOBIUM  Nb
	GOLD - AU 75%
	SILVER - AG 93%

	PLATINUM PT-93.5%
	AISI 316L
	AISI 321

	SUPERDUPLEX,SAF2507 
	17-4PH
	W6MO5CR4V2(М2)

	CoCr28V6
	COCRMO
	COCRMOW

	COCRW
	NICR
	NITINOL (NITI),

	INVAR 36
	H13
	4CR13

	TITANIUM Grade5 ( TI6AL4V),
	TITANIUM  (TA-15),
	ALUMINUM -AL6061

	AL2024
	ZL104
	ALSI10MG



Particle sizes: 0-15µ/0-45µ/15-53µ/10-63µ/50-105µ/45-150µ.[image: ][image: ][image: ]
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